{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["Grafiek1","Sjabloon Dequidt","Platenlijst","Kantenlijst","Uitleg invulblad"],"not_rendered":{"charts":2,"images":3,"defined_names":2},"unopened":[{"sheet":"Grafiek1","index":0,"reason":"not_a_worksheet"}],"read":"whole","date_system":"1900"}

{"sheet":"Sjabloon Dequidt","index":1,"n_rows":8,"n_cols":12,"rows_kept":8,"merged":[[0,0,0,13],[2,0,2,1],[2,2,2,5],[3,0,3,1],[3,2,3,5],[4,0,4,1],[4,2,4,5],[5,0,5,1],[5,2,5,5]]}
["Invulblad verzagen - kanten lijmen"]
[]
["Naam:"]
["Adres:"]
["Telefoon:"]
["E-mail:"]
[]
["POSITIE","BENAMING","MATERIAAL","AANTAL","LENGTE","BREEDTE","NERF","VOOR","ACHTER","LINKS","RECHTS","REFERENTIE"]

{"sheet":"Platenlijst","index":2,"n_rows":62,"n_cols":1,"rows_kept":62,"hidden":true}
["Platen"]
["Melamine 18 mm wit"]
["Melamine 8 mm wit"]
["MDF melamine wit 18 mm"]
["MDF bruin 3 mm"]
["MDF bruin 6 mm"]
["MDF bruin 9 mm"]
["MDF bruin 12 mm"]
["MDF bruin 15 mm"]
["MDF bruin 18 mm"]
["MDF bruin 22 mm"]
["MDF BW 18 mm"]
["MDF zwart 18 mm"]
["MDF WW 12 mm"]
["MDF WW 16 mm"]
["MDF WW 18 mm"]
["MDF WW 30 mm"]
["MDF WW 38 mm"]
["MDF WW + primer 9 mm"]
["MDF WW + primer 12 mm"]
["MDF WW + primer 15 mm"]
["MDF WW + primer 18 mm"]
["WBP multiplex 3,6 mm"]
["WBP multiplex 5,5 mm"]
["WBP multiplex 9 mm"]
["WBP multiplex 12 mm"]
["WBP multiplex 15 mm"]
["WBP mulitplex 18 mm"]
["WBP multiplex 22 mm"]
["WBP multiplex 25 mm"]
["Berken multiplex 18 mm"]
["Eliotis pine 18 mm"]
["WBP multiplex 12 mm 2de keuze"]
["WISA vuren 18 mm"]
["Poolse grenen 4 mm"]
["Poolse grenen 12 mm"]
["Poolse grenen 15 mm"]
["Poolse grenen 18 mm"]
["Unalit bruin 3,2 mm"]
["Unalit glassee 3,2 mm"]
["Volle kern 6 mm wit"]
["Forex 10 mm wit"]
["Multiplex eik 4 mm"]
["Multiplex eik 10 mm"]
["Multiplex eik 18 mm"]
["Betonplex 18 mm 1ste keuze"]
["Betonplex 18 mm Chinees"]
["Betonplex 4 mm"]
["Betonplex 8 mm"]
["Betonplex 12 mm"]
["Betonplex 15 mm"]
["Betonplex 21 mm"]
["Betonplex anti-slip 12 mm"]
["Betonplex anti-slip 18 mm"]
["Betonspan 18 mm"]
["Betonplex 18 mm wit"]
["Berken multiplex + primer 18 mm"]
["Houtvezel 8 mm"]
["Houtvezel 12 mm"]
["Houtvezel 16 mm"]
["Houtvezel 18 mm"]
["Houtvezel 22 mm"]

{"sheet":"Kantenlijst","index":3,"n_rows":9,"n_cols":1,"rows_kept":9,"hidden":true}
["Kanten"]
[]
["pvc 1 mm kleur"]
["pvc 1 mm wit"]
["pvc 1 mm kleur"]
["pvc 2 mm wit"]
["formica"]
["fineer"]
["primer"]

{"sheet":"Uitleg invulblad","index":4,"n_rows":1,"n_cols":1,"rows_kept":1,"merged":[[0,0,0,13]]}
["Uitleg invulblad"]